# SpyThreadParam Class Reference

Class used to transmit the input from the tracker to the thread which is tracking changes in the device routing table and the output from this thread to the tracker. More...

`#include <SpyThreadParam.h>`

List of all members.

## Public Member Functions

bool | get_rt_state ()
| Function used to return the device routing table status.
void | initiate_rt_state ()
| Method used to initiate the routing table status.
void | rt_is_modified ()
| Method used to track and report any changes in the device routing table.
void | set_tracking_error (char *er)
| Method used to report any error that occurs while tracker the device routing table.

## Private Attributes

bool | rt_was_modified
| Used to indicate the routing table status.
std::string | error
| Used to indicate if there was an error while tracking changes in the routing table.

## Detailed Description

Class used to transmit the input from the tracker to the thread which is tracking changes in the device routing table and the output from this thread to the tracker.

The documentation for this class was generated from the following files:

- Mes documents/Visual Studio 2005/Projects/WM-ADHOC-TRACKER/WM-ADHOC-TRACKER/SpyThreadParam.h
- Mes documents/Visual Studio 2005/Projects/WM-ADHOC-TRACKER/WM-ADHOC-TRACKER/SpyThreadParam.cpp